For 1990-2009 cars

#### Tools Required

• | J 25033-C Power Steering Pulley Installer

• | J 25034-C Power Steering Pulley Remover

### Removal Procedure

1. Remove the upper engine mount. Refer to Engine Mount Replacement in Engine Mechanical - 3.4L.
2. Remove the drive belt from the power steering pump pulley. Refer to Drive Belt Replacement in Engine Mechanical - 3.4L.
3. Remove the power steering pump. Refer to Power Steering Pump Replacement .
4. Remove the power steering pump pulley using the J 25034-C .

### Installation Procedure

1. Install the power steering pump pulley to the pump using the J 25033-C . Ensure that the face of the pulley hub is flush with the pump drive shaft.
2. Install the power steering pump. Refer to Power Steering Pump Replacement .
3. Install the drive belt to the power steering pump pulley. Refer to Drive Belt Replacement in Engine Mechanical - 3.4L.
4. Install the upper engine mount. Refer to Engine Mount Replacement in Engine Mechanical - 3.4L.
5. Fill the power steering pump with power steering fluid. Refer to Checking and Adding Power Steering Fluid .
6. Bleed the power steering system. Refer to Power Steering System Bleeding .