For 1990-2009 cars

#### Tools Required

J 42059 Cigarette Lighter Socket Remover

### Removal Procedure

1. Remove the cigarette lighter fuse.
2. Remove the cigarette lighter element.
3. Remove the cigarette lighter socket by placing one side of the "T" portion of the tool J 42059 into the tab window and then the other should be angled into the opposite tab window, then pull the lighter socket straight out.
4. Remove the tool from the lighter socket.
5. Disconnect the electrical connector from the cigarette lighter socket.
6. Remove the cigarette lighter retainer using your index finger and pulling out.

### Installation Procedure

1. Position the cigarette lighter retainer with the key to the slot into the cigarette lighter hole.
2. Install the cigarette lighter retainer pressing into place until fully seated.
3. Connect the electrical connector to cigarette lighter socket.
4. Align the cigarette lighter socket to the cigarette lighter retainer and press into place until fully seated.
5. Install the cigarette lighter fuse.
6. Install the cigarette lighter element.
7. Inspect the instrument panel lighter for proper operation.