For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
Important: A short to ground will cause an open fuse(s). Before performing this diagnostic procedure, inspect the fuse(s) for an open.
1 |

1. Turn the headlamp switch to the head position.
2. Use a test lamp in order to backprobe the turn/headlamp switch assembly connector C1 between terminal 35 and positive battery voltage.

Does the test lamp light?

--

Go to Step 2

Go to Step 3

2 | Replace the turn/headlamp switch assembly. Refer to Multifunction Turn Signal Lever Replacement - On Vehicle in Steering Wheel and Column-Standard pair complete? | -- | Go to Daytime Running Lights (DRL) System Check | --
3 | Repair the open in CKT 150 between the turn/headlamp switch assembly and ground splice pack G201. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Daytime Running Lights (DRL) System Check | --