For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Ball Joint to Steering Knuckle Nut

- First Pass

10 N·m

89 lb in

- Final Pass

+180°

Control Arm to Frame Bolts, Front Bushing

- First Pass

60 N·m

45 lb ft

- Final Pass

+180°

Control Arm to Frame Bolts, Rear Vertical Bushing

- First Pass

100 N·m

74 lb ft

- Final Pass

+180°

Hub and Bearing to Steering Knuckle Bolts | 95 N·m | 70 lb ft
Stabilizer Shaft Clamp | 66 N·m | 49 lb ft
Stabilizer Shaft Link Nuts | 17 N·m | 13 lb ft
Strut Assembly to Body Bolt | 25 N·m | 18 lb ft
Strut Assembly to Body Nuts | 25 N·m | 18 lb ft
Strut Nut to Strut Rod | 75 N·m | 55 lb ft
Strut to Steering Knuckle Nuts | 180 N·m | 133 lb ft
Suspension Crossmember Front Bolts | 245 N·m | 180 lb ft
Suspension Crossmember to Body Rear Bolts | 70 N·m | 52 lb ft
Transmission Mount Bolt | 120 N·m | 89 lb ft