For 1990-2009 cars

### Removal Procedure

1. Remove the front floor console. Refer to Front Floor Console Replacement .
2. Remove the bracket screws from the instrument panel (IP) center support bracket. Oldsmobile shown.
3. Remove the IP center support bracket. Pontiac shown.

### Installation Procedure

1. Position the IP center support bracket. Pontiac shown.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the screws to the IP center support bracket. Oldsmobile shown.

Tighten
Tighten the screws to 3 N·m (27 lb in).

3. Install the front floor console. Refer to Front Floor Console Replacement .