For 1990-2009 cars

### Removal Procedure

1. Remove the rear fascia. Refer to Rear Bumper Fascia Replacement .
2. Remove the push-pin retainers (3).
3. Remove the energy absorber (2) from the impact bar (1).

### Installation Procedure

1. Install the energy absorber (2) to the impact bar (1).
2. Install the push-pin retainers to the energy absorber (3).
3. Install the fascia. Refer to Rear Bumper Fascia Replacement .