For 1990-2009 cars

### Removal Procedure

1. Remove the screws (2) from the fuel tank filler pocket.
2. Remove the gas cap.
3. Remove the fuel tank filler pocket (1).

### Installation Procedure

1. Install the fuel tank filler pocket (1).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolts (2) to the fuel tank filler pocket.

Tighten
Tighten the fuel tank filler pocket bolts to 2 N·m (18 lb in).

3. Install the gas cap.