For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the front door water deflector, starting at the top and pull downward (1).
3. Route the electrical connectors (and inside handle rod) through the existing holes in the water deflector.

### Installation Procedure

1. Route the electrical connectors (and inside handle rod) through the water deflector.
2. Install the front door water deflector (1) to the door, pressing into place until fully seated.
3. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement .