For 1990-2009 cars

## Steering Gear Rack Bearing Preload Adjustment - Off Vehicle Rack and Pinion

1. Loosen the adjuster plug lock nut (1).

Notice: Refer to Fastener Notice in the Preface section.

2. Tighten the adjuster plug.

Tighten

• | Tighten to 15 N·m (11 lb ft)

• | Turn the adjuster plug back 30 degrees.

3. Install the adjuster plug lock nut (1) to the adjuster plug.

Tighten
Hold the adjuster plug stationary while tightening the adjuster plug lock nut (1) to 68 N·m (50 lb ft).