For 1990-2009 cars

Table 1: | Auxiliary Power Outlet (Oldsmobile)
Table 2: | Cigar Lighter
Table 3: | Ignition Switch C1
Table 4: | Ignition Switch C2
Table 5: | LH IP Junction Block, C1
Table 6: | LH IP Junction Block, C2
Table 7: | LH IP Junction Block, C3
Table 8: | RH IP Junction Block, C1
Table 9: | RH IP Junction Block, C2
Table 10: | RH IP Junction Block, C3
Table 11: | Underhood Junction Block C1 (LD9 Only)
Table 12: | Underhood Junction Block C1 (LA1 Only)
Table 13: | Underhood Junction Block C2
Table 14: | Underhood Junction Block C3
Table 15: | Underhood Junction Block C4
Table 16: | Underhood Junction Block C5
Table 17: | Underhood Junction Block C6
Table 18: | Underhood Junction Block C7

#### Auxiliary Power Outlet (Oldsmobile)

Connector Part Information |

• | 12047699

• | 2-Way Mixed Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 40 | Fuse Output, Battery
B | BLK | 150 | Ground

#### Cigar Lighter

Connector Part Information |

• | 12176836

• | 3-Way F Metri-Pack 280 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 40 | Fuse Output, Battery
B | -- | -- | Not Used
C | BLK | 150 | Ground

#### Ignition Switch C1

Connector Part Information |

• | 12110075

• | 6-Way F Metri-Pack Mixed Series (NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED | 242 | Fuse Output, Battery
B | YEL | 5 | Ignition Switch Output (CRANK)
C | ORN | 300 | Ignition Switch Output (Ignition 3)
C | ORN | 300 | Ignition Switch Output (Ignition 3)
D | LT GRN | 80 | Key Reminder Switch Signal
E | DK GRN | 500 | Ignition Switch Output (ACCY, RUN, CRANK)
F | -- | -- | Not Used

#### Ignition Switch C2

Connector Part Information |

• | 12162229

• | 6-Way F Metri-Pack Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED | 842 | Fuse Output, Battery
B | PNK | 3 | Ignition Switch Output (Ignition 1)
B | PNK | 3 | Ignition Switch Output (Ignition 1)
C | BRN | 4 | Ignition Switch Output (ACCY)
D | -- | -- | Not Used
E | BLK/WHT | 151 | Ground-Clean
F | -- | -- | Not Used

#### LH IP Junction Block, C1

Connector Part Information |

• | 12193962

• | 68-Way F Metri-Pack 280 Series (BRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | -- | -- | Not Used
A2 | BRN | 4 | Ignition Switch Output (ACCY)
A3 | PPL | 1807 | Serial Data Signal, Class B, 10400 Baud (Primary)
A3 | PPL | 1807 | Serial Data Signal, Class B, 10400 Baud (Primary)
A4 | PNK | 3 | Ignition Switch Output (Ignition 1)
A5-A6 | -- | -- | Not Used
A7 | DK GRN | 500 | Ignition Switch Output (ACCY, RUN, CRANK)
A8-A11 | -- | -- | Not Used
A12 | ORN | 1440 | Fuse Output, Battery
A12 | ORN | 1440 | Fuse Output, Battery
B1 | YEL | 43 | Fuse Output, ACCY
B2 | YEL | 143 | Fuse Output, ACCY
B3 | -- | -- | Not Used
B4 | PNK | 739 | Fuse Output, Ignition 1
B5 | -- | -- | Not Used
B6 | YEL | 1139 | Fuse Output, Ignition 1, SIR
B7 | PPL | 1500 | Fuse Output, Ignition 0
B8 | -- | -- | Not Used
B9 | PPL | 1600 | Fuse Output, Ignition 0
B9 | PPL | 1600 | Fuse Output, Ignition 0
B10 | -- | -- | Not Used
B11 | ORN | 1440 | Fuse Output, Battery
B12 | -- | -- | Not Used
C1 | -- | -- | Not Used
C2 | YEL | 143 | Fuse Output, ACCY
C3-C4 | -- | -- | Not Used
C5 | RED | 442 | Fuse Output, Battery
C8-C9 | -- | -- | Not Used
C10 | YEL | 356 | Power Door Lock Relay Feed-Coil (Driver Door Unlock)
C11 | -- | -- | Not Used
C12 | ORN | 1140 | Fuse Output, Battery
D1 | YEL | 243 | Fuse Output, ACCY (Pontiac Only)
D2 | PPL | 1807 | Serial Data Signal, Class B, 10400 Baud (Primary)
D2 | PPL | 1807 | Serial Data Signal, Class B, 10400 Baud (Primary)
D3-D12 | -- | -- | Not Used
E1 | BLK/WHT | 151 | Ground-Clean
E2 | -- | -- | Not Used
E3 | PPL | 1807 | Serial Data Signal, Class B, 10400 Baud (Primary)
E3 | PPL | 1807 | Serial Data Signal, Class B, 10400 Baud (Primary)
E4 | LT BLU/BLK | 14 | Turn Signal Lamp Feed-LF
E4 | LT BLU/BLK | 14 | Turn Signal Lamp Feed-LF
E5-E6 | -- | -- | Not Used
E7 | ORN | 1540 | Fuse Output, Battery
E8 | -- | -- | Not Used
E9 | ORN | 1732 | Electronic Control Unit Output-12 Volt (Inadvertent Load Control)
E9 | ORN | 1732 | Electronic Control Unit Output-12 Volt (Inadvertent Load Control)
E10 | BLK | 150 | Ground
E11 | -- | -- | Not Used
E12 | RED | 642 | Fuse Output, Battery
F1 | PNK/BLK | 1379 | Oil Change Reset Switch Signal
F2 | WHT | 156 | Courtesy Lamp Output
F2 | WHT | 156 | Courtesy Lamp Output
F3 | LT BLU | 1344 | Trunk Release Relay Output-Coil
F4-F7 | -- | -- | Not Used
F8 | WHT | 194 | Power Door Lock Relay Feed-Unlock Coil
F9 | -- | -- | Not Used
F10 | LT BLU | 195 | Power Door Lock Relay Feed-lock Coil
F11-F12 | -- | -- | Not Used

#### LH IP Junction Block, C2

Connector Part Information |

• | 12176739

• | 30-Way F Metri-Pack 280 Series (TAN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | LT BLU | 20 | Stop Lamp Feed
A2 | WHT | 156 | Courtesy Lamp Output
A2 | WHT | 156 | Courtesy Lamp Output
A3 | LT BLU/BLK | 14 | Turn Signal Lamp Feed LF
A3 | LT BLU/BLK | 14 | Turn Signal Lamp Feed LF
A4-A12 | -- | -- | Not Used
B1-B3 | -- | -- | Not Used
B4 | LT GRN/BLK | 394 | Door Handle Switch Signal, Left Front
B5 | TAN | 201 | Speaker Feed, Left Front
B8-B9 | -- | -- | Not Used
B10 | GRY | 120 | Fuel Pump Motor Feed
B11 | -- | -- | Not Used
B12 | PPL | 420 | Brake Pedal Switch Output (TCC)
C1 | BLK | 293 | Rear Defogger Element Feed
C2 | BRN | 241 | Fuse Output, Ignition 3
C3 | -- | -- | Not Used
C4 | DK GRN/WHT | 1135 | Brake Transaxle Shift Interlock Solenoid Feed
C5 | GRY | 118 | Speaker Return, Left Front
C8 | BLK | 1576 | Trunk Release Switch Output
C9 | ORN | 1732 | Electronic Control Unit Output-12 Volt (Inadvertent Load Contrrol)
C10 | BRN | 199 | Speaker Feed, LR
C11 | -- | -- | Not Used
C12 | YEL | 116 | Speaker Return, LR

#### LH IP Junction Block, C3

Connector Part Information |

• | 12176740

• | 30-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | ORN | 140 | Fuse Output, Battery
A2 | GRY | 295 | Power Door Lock Motor Feed (LOCK)
A2 | GRY | 295 | Power Door Lock Motor Feed (LOCK)
A3 | -- | -- | Not Used
A4 | TAN | 294 | Power Door Lock Motor Feed (UNLOCK)
A5 | -- | -- | Not Used
A8 | ORN | 540 | Fuse Output, Battery
A9 | BLK/WHT | 56 | Trunk Release Motor Feed
A10 | LT BLU/BLK | 14 | Turn Signal Lamp Feed, LF
A11 | WHT | 156 | Courtesy Lamp Output
A12 | LT BLU | 20 | Stoplamp Feed
B1 | PPL | 420 | Brake Pedal Switch Output (TCC)
B2 | GRY | 295 | Power Door Lock Motor Feed (LOCK)(Sedan Only)
B2 | GRY | 295 | Power Door Lock Motor Feed (LOCK)(Sedan Only)
B3 | GRY | 120 | Fuel Pump Motor Feed
B4 | TAN | 294 | Power Door Lock Motor Feed (UNLOCK)(Sedan Only)
B4 | TAN | 294 | Power Door Lock Motor Feed (UNLOCK)(Sedan Only)
B5 | ORN | 1040 | Fuse Output, Battery (w/AUO)
B5 | ORN | 1040 | Fuse Output, Battery (w/AUO & UQ3)
B8 | TAN | 201 | Speaker Feed, Left Front
B9 | LT GRN/BLK | 394 | Door Handle Switch Signal, Left Front
B10 | ORN | 1840 | Fuse Output, Battery
B11 | LT BLU | 20 | Stoplamp Feed
B12 | LT BLU | 20 | Stoplamp Feed
C1 | YEL | 116 | Speaker Return, LR
C1 | YEL | 116 | Speaker Return, LR (w/UQ3)
C2 | TAN | 694 | Power Door Lock Motor Feed-Driver Door Unlock
C3 | BRN | 199 | Speaker Feed, LR
C3 | BRN | 199 | Speaker Feed, LR (w/UQ3)
C4 | ORN | 1732 | Electronic Control Unit-12 Volt (Inadvertent Load Control)
C4 | ORN | 1732 | Electronic Control Unit-12 Volt (Inadvertent Load Control)
C5 | BLK | 1576 | Trunk Release Switch Signal
C8 | GRY | 118 | Speaker Return, Left Front
C9 | DK GRN/WHT | 1135 | Brake Transaxle Shift Interlock Solenoid Feed
C10 | LT BLU | 20 | Stoplamp Feed
C11 | BRN | 241 | Fuse Output, Ignition 3
C12 | BLK | 293 | Rear Defogger Element Feed

#### RH IP Junction Block, C1

Connector Part Information |

• | 12193962

• | 68-Way F Metri-Pack 280 Series (TAN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | ORN | 1740 | Fuse Output, Battery
A2 | ORN | 340 | Fuse Output, Battery
A3-A4 | -- | -- | Not Used
A5 | BRN | 641 | Fuse Output, Ignition 3
A6 | -- | -- | Not Used
A7 | BRN | 1244 | IP Lamp Feed
A8-B1 | -- | -- | Not Used
B2 | RED | 1042 | Fuse Output, Battery
B3 | -- | -- | Not Used
B4 | BRN | 341 | Fuse Output, Ignition 3
B5 | -- | -- | Not Used
B6 | BRN | 441 | Fuse Output, Ignition 3
B7 | GRY | 8 | IP Lamp Feed
B8-B11 | -- | -- | Not Used
B12 | BRN | 9 | Park Lamp Feed
B12 | BRN | 9 | Park Lamp Feed
C1-C3 | -- | -- | Not Used
C4 | BRN | 341 | Fuse Output, Ignition 3
C5 | ORN | 300 | Ignition Switch Output (Ignition 3)
C8-C11 | -- | -- | Not Used
C12 | BRN | 9 | Park Lamp Feed
D1-D12 | -- | -- | Not Used
E1 | -- | -- | Not Used
E2 | DK BLU | 15 | Turn Signal Lamp Feed, Right Front
E2 | DK BLU | 15 | Turn Signal Lamp Feed, Right Front
E3-E5 | -- | -- | Not Used
E6 | GRY | 8 | IP Lamp Feed
E6 | GRY | 8 | IP Lamp Feed
E7 | GRY | 8 | IP Lamp Feed
E8-E11 | -- | -- | Not Used
E12 | YEL | 32 | Park Lamp Feed
F1 | -- | -- | Not Used
F1 | -- | -- | Not Used
F2 | DK BLU | 15 | Turn Signal Lamp Feed, Right Front
F2 | DK BLU | 15 | Turn Signal Lamp Feed, Right Front
F3 | DK GRN/WHT | 1317 | Fog Lamp Relay Output-Coil
F4 | PPL | 34 | Fog Lamp Feed (w/T37)
F4 | PPL | 34 | Fog Lamp Feed (w/T37)
F5-F6 | -- | -- | Not Used
F7 | GRY | 8 | IP Lamp Feed
F8-F11 | -- | -- | Not Used
F12 | BRN | 9 | Park Lamp Feed
F12 | BRN | 9 | Park Lamp Feed

#### RH IP Junction Block, C2

Connector Part Information |

• | 12176741

• | 30-Way F Metri-Pack 280 Series (BRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | -- | -- | Not Used
A2 | DK GRN | 145 | Power Antenna Relay Feed-Coil (Oldsmobile)
A3 | DK GRN | 117 | Speaker Return, Right Front
A4-A12 | -- | -- | Not Used
B1 | BLK/WHT | 238 | Seat Belt Switch Signal
B2 | -- | -- | Not Used
B3 | DK BLU | 46 | Speaker Feed, Right Rear
B4 | -- | -- | Not Used
B5 | -- | -- | Not Used
B8 | GRY | 8 | IP Lamp Feed
B8 | GRY | 8 | IP Lamp Feed
B9 | WHT | 682 | Lock Switch Signal
B10 | LT GRN | 377 | RFA Data Link
B11 | LT GRN | 24 | Backup Lamp Feed
B12 | -- | -- | Not Used
C1 | LT GRN | 200 | Speaker Feed, Right Front
C2 | LT BLU | 395 | Door Handle Switch Signal-RF
C3 | LT BLU | 115 | Speaker Return, Right Rear
C4-C8 | -- | -- | Not Used
C9 | LT BLU | 1134 | Park Brake Switch Signal
C10-C12 | -- | -- | Not Used

#### RH IP Junction Block, C3

Connector Part Information |

• | 12176740

• | 30-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | BRN | 9 | Park Lamp Feed
A2 | BRN | 9 | Park lamp Feed (Oldsmobile Only)
A3 | BRN | 9 | Park lamp Feed (Oldsmobile Only)
A4 | LT GRN | 24 | Backup Lamp Feed
A5 | DK BLU | 15 | Turn Signal Lamp Feed, Right Front
A8 | BRN | 141 | Fuse Output, Ignition 3
A9 | BRN | 341 | Fuse Output, Ignition 3
A10 | DK GRN | 117 | Speaker Return, Right Front
A11 | DK GRN | 145 | Power Antenna Relay Feed-Coil (Oldsmobile Only)
A12 | BRN | 541 | Fuse Output, Ignition 3
B1 | BRN | 9 | IP Lamp Feed
B2 | LT GRN | 24 | Backup Lamp Feed
B3 | LT GRN | 377 | RFA Data Link
B4 | WHT | 682 | Power Door Lock Switch Signal
B4 | WHT | 682 | Power Door Lock Switch Signal
B5 | GRY | 8 | IP Lamp Feed (w/Power Mirrors) (Oldsmobile Only)
B8 | BRN | 141 | Fuse Output, Ignition 3 (w/Power Windows)
B9 | DK BLU | 46 | Speaker Feed, Right Rear
B10 | DK BLU | 46 | Speaker Feed, Right Rear
B11 | LT BLU | 395 | Rear Door Jamb Switch Signal
B11 | LT BLU | 395 | Rear Door Jamb Switch Signal
B12 | BLK/WHT | 238 | Seat Belt Switch Signal
C1 | BRN | 9 | Park Lamp Feed
C2 | LT GRN | 24 | Backup Lamp Feed (Pontiac)
C3 | LT GRN | 24 | Backup Lamp Feed
C4 | LT BLU | 1134 | Park Brake Switch Signal
C5 | GRY | 8 | IP Lamp Feed
C5 | GRY | 8 | IP Lamp Feed
C6-C8 | -- | -- | Not Used
C9 | LT BLU | 115 | Speaker Return, Right Rear
C10 | LT BLU | 115 | Speaker Return, Right Rear
C11 | LT BLU | 395 | Door Handle Switch Signal Right Front
C12 | LT GRN | 200 | Speaker Feed, Right Front

#### Underhood Junction Block C1 (LD9 Only)

Connector Part Information |

• | 15303512

• | 68-Way F Metri-Pack 280 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | ORN | 855 | Fuse Output, ABS
A2 | DK GRN/WHT | 459 | A/C Compressor Control Relay Output-Coil
A3 | PNK | 1632 | ABS Enable Relay Output-Coil
A4 | PNK | 1039 | Fuse Output, Ignition 1
A5 | -- | -- | Not Used
A6 | GRY | 729 | A/C Compressor Clutch Solenoid Output
A7-A8 | -- | -- | Not Used
A9 | LT BLU/BLK | 396 | Cruise Control Signal, Engaged
A11 | YEL | 5 | Ignition Switch Output (CRANK)
A10 | -- | -- | Not Used
A12 | LT BLU | 20 | Stoplamp Feed
B1 | ORN | 855 | Fuse Output, ABS
B2 | -- | -- | Not Used
B3 | RED | 1633 | ABS Enable Relay Output (N.O. Contact)
B4 | DK GRN | 83 | Cruise Control Signal, Disengage
B5 | PNK | 139 | Fuse Output, Ignition 1
B6 | DK GRN | 59 | A/C Compressor Clutch Solenoid Feed
B7 | -- | -- | Not Used
B8 | BLK | 450 | Ground
B9-B12 | -- | -- | Not Used
C1 | ORN | 855 | Fuse Output, Ignition 1
C2 | -- | -- | Not Used
C3 | PPL | 420 | Brake Pedal Switch Output, TCC
C4 | GRY | 120 | Fuel Pump Motor Feed
C8 | PNK | 639 | Fuse Output, Ignition 1
C9 | -- | -- | Not Used
C10 | GRY | 532 | Coolant Fan Motor Feed (Secondary)
C11-C12 | -- | -- | Not Used
D1-D2 | -- | -- | Not Used
D3 | DK GRN | 335 | Coolant Fan Relay Output-Coil
D4 | GRY | 120 | Fuel Pump Motor Feed
D5 | PNK | 239 | Fuse Output, Ignition 1
D8 | -- | -- | Not Used
D9 | BRN | 241 | Fuse Output, Ignition 3
D10 | BLK | 450 | Ground
D11 | DK BLU | 473 | Coolant Fan Relay Output-Coil (Secondary)
D12 | -- | -- | Not Used
E1 | ORN | 1640 | Fuse Output, Battery
E2-E3 | -- | -- | Not Used
E4 | GRY | 120 | Fuel Pump Motor Feed
E5 | -- | -- | Not Used
E6 | ORN | 480 | Fuse Output, Electronic Control Unit
E7 | ORN | 840 | Fuse Output, Battery
E8 | DK GRN/WHT | 465 | Fuel Pump Relay Feed-Coil
E9-E12 | -- | -- | Not Used
F1-F2 | -- | -- | Not Used
F3 | LT BLU | 409 | Coolant Fan Motor Feed
F4 | GRY | 120 | Fuel Pump Motor Feed
F5 | PNK | 539 | Fuse Output, Ignition 1
F6-F8 | -- | -- | Not Used
F9 | BRN | 241 | Fuse Output, Ignition 3
F10 | -- | -- | Not Used
F11 | WHT | 504 | Coolant Fan Motor Output (Secondary)
F12 | -- | -- | Not Used

#### Underhood Junction Block C1 (LA1 Only)

Connector Part Information |

• | 15303512

• | 68-Way F Metri-Pack 280 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | ORN | 855 | Fuse Output, ABS
A2 | DK GRN/WHT | 459 | A/C Compressor Control Relay Output-Coil
A3 | PNK | 1632 | ABS Enable Relay Output-Coil
A4 | PNK | 1039 | Fuse Output, Ignition 1
A5 | -- | -- | Not Used
A6 | GRY | 729 | A/C Compressor Clutch Solenoid Output
A7 | PNK | 839 | Fuse Output, Ignition 1
A8 | -- | -- | Not Used
A9 | LT BLU/BLK | 396 | Cruise Control Signal-Engaged
A10 | -- | -- | Not Used
A11 | YEL | 5 | Ignition Switch Output (CRANK)
A12 | LT BLU | 20 | Stoplamp Feed
B1 | ORN | 855 | Fuse Output, ABS
B2 | -- | -- | Not Used
B3 | RED | 1633 | ABS Enable Relay Output-N.O. Contact
B4 | DK GRN | 83 | Cruise Control Signal-Disengage
B5 | PNK | 139 | Fuse Output, Ignition 1
B6 | DK GRN | 59 | A/C Compressor Clutch Solenoid Feed
B7 | -- | -- | Not Used
B8 | BLK | 450 | Ground
B9-B11 | -- | -- | Not Used
B12 | BLK | 450 | Ground
C1 | ORN | 855 | Fuse Output, Ignition 1
C2 | -- | -- | Not Used
C3 | PPL | 420 | Brake Pedal Switch Output, TCC
C4-C5 | -- | -- | Not Used
C8 | PNK | 639 | Fuse Output, Ignition 1
C9 | -- | -- | Not Used
C10 | GRY | 532 | Coolant Fan Motor Feed (Secondary)
C11 | -- | -- | Not Used
C12 | BLK | 450 | Ground
D1-D2 | -- | -- | Not Used
D3 | DK GRN | 335 | Coolant Fan Relay Output-Coil
D4 | -- | -- | Not Used
D5 | PNK | 239 | Fuse Output, Ignition 1
D8 | PNK | 639 | Fuse Output, Ignition 1
D9 | BRN | 241 | Fuse Output, Ignition 3
D10 | BLK | 450 | Ground
D11 | DK BLU | 473 | Coolant Fan Relay Output-Coil (Secondary)
D12 | -- | -- | Not Used
E1 | ORN | 1640 | Fuse Output, Battery
E2 | BRN | 436 | AIR Relay (California Emmissions Only)
E3-E5 | -- | -- | Not Used
E6 | ORN | 480 | Fuse Output, Electronic Control Unit
E7 | ORN | 840 | Fuse Output, Battery
E8 | DK GRN/WHT | 465 | Fuel Pump Relay Feed-Coil
E9 | BRN | 241 | Fuse Output, Ignition 3
E10-E12 | -- | -- | Not Used
F1-F2 | -- | -- | Not Used
F3 | LT BLU | 409 | Coolant Fan Motor Feed
F4 | -- | -- | Not Used
F5 | PNK | 539 | Fuse Output, Ignition 1
F6-F8 | -- | -- | Not Used
F9 | BRN | 241 | Fuse Output, Ignition 3
F10 | -- | -- | Not Used
F11 | WHT | 504 | Coolant Fan Motor Output (Secondary)
F12 | -- | -- | Not Used

#### Underhood Junction Block C2

Connector Part Information |

• | 15303513

• | 68-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | BRN | 341 | Fuse Output, Ignition 3
A2-A12 | -- | -- | Not Used
B1-B4 | -- | -- | Not Used
B5 | BRN | 9 | Park Lamp Feed
B5 | BRN/WHT | 9 | Side Marker Lamp Feed
B6-B8 | -- | -- | Not Used
B9 | BRN | 9 | Park Lamp Feed
B9 | BRN/WHT | 9 | Side Marker Lamp Feed
B10 | DK BLU | 15 | Turn Signal Lamp Feed, Right Front
B10 | DK BLU | 15 | Side Marker Lamp Feed
B11 | -- | -- | Not Used
B12 | LT BLU | 20 | Stoplamp Feed
C1 | -- | -- | Not Used
C2 | DK BLU | 1201 | Headlamp Output, Low Beam
C2 | DK BLU | 1201 | Headlamp Output, Low Beam
C3 | PPL | 420 | Brake Pedal Switch Output, TCC
C4-C8 | -- | -- | Not Used
C9 | BRN | 9 | Park Lamp Feed
C9 | BRN | 9 | Park Lamp Feed
C10 | LT BLU/BLK | 14 | Turn Signal Lamp Feed, Left Front
C10 | LT BLU/BLK | 14 | Turn Signal Lamp Feed, Left Front
C11 | -- | -- | Not Used
C12 | DK GRN | 29 | Horn Feed
D1-D9 | -- | -- | Not Used
D10 | ORN | 740 | Fuse Output, Battery (Oldsmobile Only)
D11-E2 | -- | -- | Not Used
E3 | RED | 78 | AIR Pump Motor (California Emissions Only)
E4 | DK GRN | 83 | Cruise Control Signal, Disengage
E5-E7 | -- | -- | Not Used
E8 | ORN | 640 | Fuse Output, Battery
E9-E12 | -- | -- | Not Used
F1-F3 | -- | -- | Not Used
F4 | PPL | 34 | Fog Lamp Feed
F4 | PPL | 34 | Fog Lamp Feed
F5 | LT BLU/BLK | 396 | Cruise Control Signal, Engaged
F6 | PNK | 1200 | Headlamp Lamp Output (High Beam)
F6 | PNK | 1200 | Headlamp Lamp Output (High Beam)
F7 | -- | -- | Not Used
F8 | ORN | 640 | Fuse Output, Battery (Oldsmobile Only)
F9-F11 | -- | -- | Not Used
F12 | DK BLU | 593 | High Beam Headlamp Feed-Daytime Running Lamps

#### Underhood Junction Block C3

Connector Part Information |

• | 15328719

• | 68-Way F Metri-Pack 280 Series (BRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | ORN | 40 | Fuse Output, Battery
A2-A3 | -- | -- | Not Used
A4 | WHT | 193 | Rear Defogger Relay Output-Coil
A5 | PPL | 34 | Fog Lamp Feed
A6 | ORN | 300 | Ignition Switch Output (Ignition 3)
A7 | BRN | 241 | Fuse Output, Ignition 3
A8 | -- | -- | Not Used
A9 | PNK/WHT | 1970 | Low Beam Headlamp Relay Output-Coil
A10 | BLK | 150 | Ground
A11 | BRN | 41 | Fuse Output, Ignition 3
A11 | BRN | 41 | Fuse Output, Ignition 3
A12 | -- | -- | Not Used
B1-B2 | -- | -- | Not Used
B3 | DK GRN | 306 | Headlamp Switch Output (Headlamps OFF)
B4 | -- | -- | Not Used
B5 | BRN | 9 | Park Lamp Feed
B6 | -- | -- | Not Used
B7 | PNK | 1200 | Headlamp Lamp Output (High Beam)
B7 | PNK | 1200 | Headlamp Lamp Output (High Beam)
B8 | WHT | 1080 | Parklamp Relay Output-Coil
B9 | PPL | 65 | Blower Motor Feed
B10-B11 | -- | -- | Not Used
B12 | LT GRN/BLK | 592 | DRL Relay Output-Coil
C1-C3 | -- | -- | Not Used
C4 | PNK | 439 | Fuse Output, Ignition 1
C5 | BLK | 293 | Rear Defogger Element Feed
C8 | DK BLU | 15 | Turn Signal Lamp Feed, Right Front
C9 | LT BLU/BLK | 14 | Turn Signal Lamp Feed, Left Front
C10 | DK BLU | 101 | Blower Resistor Output
C11 | -- | -- | Not Used
C12 | BLK | 28 | Horn Relay Output
C12 | BLK | 28 | Horn Relay Output
D1 | DK BLU | 1201 | Headlamp Lamp Output, Low Beam
D1 | DK BLU | 1201 | Headlamp Lamp Output, Low Beam
D2 | BRN | 341 | Fuse Output, Ignition 3
D3-D4 | -- | -- | Not Used
D5 | PNK | 3 | Fuse Output, Ignition 1
D8 | ORN | 240 | Fuse Output, Battery
D9 | ORN | 52 | Blower Switch Output (HIGH)
D10-D12 | -- | -- | Not Used
E1-E5 | -- | -- | Not Used
E6 | GRY | 120 | Fuel Pump Motor Feed
E7-E12 | -- | -- | Not Used
F1-F2 | -- | -- | Not Used
F3 | PPL | 420 | Brake Pedal Switch Output, TCC
F4-F10 | -- | -- | Not Used
F11 | YEL | 5 | Ignition Switch Output (CRANK)
F12 | LT BLU | 20 | Stoplamp Feed

#### Underhood Junction Block C4

Connector Part Information |

• | 12146038

• | 2-Way F Metri-Pack 800 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED | 842 | Fuse Output, Battery
B | RED/BLK | 242 | Fuse Output, Battery

#### Underhood Junction Block C5

Connector Part Information |

• | 12160605

• | 2-Way F Metri-Pack 800 Series (GRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | RED | 442 | Fuse Output, Battery

#### Underhood Junction Block C6

Connector Part Information |

• | 12146037

• | 2-Way F Metri-Pack 800 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | RED | 642 | Fuse Output, Battery

#### Underhood Junction Block C7

Connector Part Information |

• | 12160606

• | 2-Way F Metri-Pack 800 Series (BRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | RED | 1042 | Fuse Output, Battery