For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle on a hoist. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the tire and wheel assemblies. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
3. Remove the stabilizer shaft links from the control arms. Refer to Stabilizer Shaft Link Replacement in Front Suspension.
4. Remove the tie rod ends from the steering knuckle. Refer to Rack and Pinion Outer Tie Rod End Replacement .
5. Remove the intermediate steering shaft from the steering gear. Refer to Intermediate Steering Shaft Replacement in Steering Wheel and Column.
6. Remove the stabilizer shaft. Refer to Stabilizer Shaft Replacement in Front Suspension.
7. Remove the power steering hoses from the from the power steering gear. Refer to the following procedures:

• | Power Steering Pressure Pipe/Hose Replacement

• | Power Steering Return Hose Replacement

8. Remove the power steering gear bolts (2) from the frame (3).
9. Remove the power steering gear (1) through the left wheel opening.

### Installation Procedure

1. Position the power steering gear (1) on the vehicle.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the power steering gear mounting bolts (2) to the frame (3).

Tighten
Tighten the bolts to 110 N·m (81 lb ft).

3. Install the power steering hoses to the power steering gear. Refer to the following procedures:

• | Power Steering Pressure Pipe/Hose Replacement

• | Power Steering Return Hose Replacement .

4. Install the stabilizer shaft. Refer to Stabilizer Shaft Replacement in Front Suspension.
5. Install the intermediate steering shaft to the steering gear. Refer to Intermediate Steering Shaft Replacement in Steering Wheel and Column.
6. Install the tie rod ends to the steering knuckle. Refer to Rack and Pinion Outer Tie Rod End Replacement .
7. Install the stabilizer shaft links to the control arms. Refer to Stabilizer Shaft Link Replacement in Front Suspension.
8. Install the tire and wheel assemblies. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
9. Lower the vehicle.
10. Bleed the air from the power steering system. Refer to Power Steering System Bleeding .