For 1990-2009 cars

#### Tools Required

J 9886-01 Door Handle Clip Remover

### Removal Procedure

1. Note the position of the window regulator handle with the window in the full up position.
2. Remove the spring clip by inserting J 9886-01 between the regulator handle and the bearing plate.
3. Pull outward on the regulator handle in order to remove the handle.
4. Remove the bearing plate from the door trim panel.

### Installation Procedure

1. Position the window to the full up position.
2. Install the bearing plate to the door trim panel.
3. Install the clip to the regulator handle.
4. Position the regulator handle to the noted position.
5. Install the regulator handle, pressing into place until fully seated.