For 1990-2009 cars

### Removal Procedure

1. Unhook the sunshade from the anchor.
2. Use a flat-bladed tool in order to push upward on the service tab until the tab recesses into the anchor.
3. Pull down and remove the sunshade anchor.

### Installation Procedure

1. From inside the anchor, push down on the retaining tab until it extends below the anchor (3).
2. Position the anchor flush to the headliner.
3. Push up on the tab until it is flush with the anchor. This will lock the anchor in place.