For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement in Seats.
2. Remove the split folding seat back, if equipped. Refer to Rear Split Folding Seat Back Replacement in Seats.
3. Remove the stationary seat back , if equipped. Refer to Rear Seat Back Replacement in Seats.
4. Pull out the door weatherstrip, if necessary.
5. Start at the top of the lower quarter trim panel. Pull the trim panel away from the quarter panel to disengage the retaining clips.
6. Remove the remainder of the trim panel from the quarter panel.

### Installation Procedure

1. Align the trim panel to the quarter panel.
2. Press the trim panel into the quarter panel until the retaining clips are fully engaged.
3. Install the door weatherstrips, if necessary.
4. Install the stationary seat back , if equipped. Refer to Rear Seat Back Replacement in Seats.
5. Install the split folding seat back, if equipped. Refer to Rear Split Folding Seat Back Replacement in Seats.
6. Install the seat cushion. Refer to Rear Seat Cushion Replacement .