For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the console. Refer to Front Floor Console Replacement in Instrument Panel, Gauges and Console.
3. Lift up on the cable retainers.
4. Disconnect the cable ends from the shifter.
5. Depress the locking tabs and remove the forward cable from the anchor.
6. On the transmission end, disconnect the cable from the shift actuator.
7. Remove both cables from the underhood cable bracket.
8. Position the passenger front carpet aside. Refer to Front Floor Panel Carpet Replacement in Interior Trim.
9. Remove the right rear floor duct elbow.
10. Separate the grommet from the floor plan.
11. Pull the cables through the passenger floor opening.

### Installation Procedure

1. Feed the cable assembly through the passenger floor pan opening.
2. Install the grommet flush with the floor opening.
3. Install the right rear floor side elbow duct.
4. Position and install the passenger side carpet. Refer to Front Floor Panel Carpet Replacement in Interior Trim.
5. Install the cables into the underhood bracket.
6. Connect the shift cable to the shift actuator.
7. Connect the cables to the shifter.
8. Press down on the locking tabs.
9. Install the console. Refer to Front Floor Console Replacement in Instrument Panel, Gauges, and Console.
10. Connect the battery.