For 1990-2009 cars

### Removal Procedure

The one-piece formed headliner consists of a molded substrate that is covered with a foam-backed cloth facing. Attach the headliner through installing the related hardware.

1. Remove the center pillar upper trim panel. Refer to Center Pillar Upper Trim Panel Replacement .
2. Remove the windshield side upper garnish moldings. Refer to Upper Pillar Garnish Molding Replacement .
3. Remove the coat hooks. Refer to Coat Hook Replacement .
4. Remove the roof rail assist handles. Refer to Assist Handle Replacement .
5. Remove the sunshades. Refer to Sunshade Replacement .
6. Remove the dome lamp (1). Refer to Dome Lamp Replacement .
7. Remove the rear quarter upper trim panels. Refer to Rear Quarter Upper Trim Panel Replacement .
8. Disconnect the wire harness connectors from the headliner.
9. Remove the rear retainers from the headliner.
10. Remove the headliner from the vehicle.

### Installation Procedure

1. Install the headliner to the vehicle.
2. Install the rear retainer to the headliner.
3. Connect the wire harness connectors to the headliner.
4. Install the rear quarter upper trim panels. Refer to Rear Quarter Upper Trim Panel Replacement .
5. Install the dome lamp (1). Refer to Dome Lamp Replacement .
6. Install the sunshades. Refer to Sunshade Replacement .
7. Install the roof rail assist handles. Refer to Assist Handle Replacement .
8. Install the coat hooks. Refer to Coat Hook Replacement .
9. Install the windshield side upper garnish moldings. Refer to Upper Pillar Garnish Molding Replacement .
10. Install the center pillar upper trim panel. Refer to Center Pillar Upper Trim Panel Replacement .