For 1990-2009 cars

• | Inspect the condition of all hoses and clamps:

- | Inspect the hoses for flexibility and no signs of bulging.

- | Inspect the hoses for cracks, cuts, kinks and areas of possible leaks.

- | Inspect the brackets, supports, ties and clamps.

- | Replace and adjust the hoses and clamps as needed.

• | Clean the front face of the radiator annually.

- | Clean the front face of the condenser.

| Important: Do not brush the radiator fins. The radiator fins are necessary for good heat transfer. Brushing damages the fins and reduces heat transfer.

| Important: Keep the front of the radiator clear for proper cooling.

- | Remove bugs, leaves, and other foreign material by blowing compressed air through the radiator.

- | Blow the air from the rear toward the front. If compressed air is not available, use a water hose in order to force water through the radiator.

- | Use water only with the engine not running and cool.