For 1990-2009 cars

### Removal Procedure

1. Loosen the vent hose clamp at the air cleaner resonator.
2. Loosen the air cleaner intake duct clamp at the air cleaner outlet resonator.
3. Loosen the air cleaner outlet resonator to throttle body clamp, located forward of the accelerator cable bracket.
4. Remove the air cleaner resonator to accelerator bracket bolt.
5. Remove the resonator from the throttle body, the air cleaner intake duct and the vent hose.

### Installation Procedure

1. Install the resonator to the throttle body, the air cleaner intake duct and the vent hose.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the air cleaner resonator to accelerator bracket bolt.

Tighten
Tighten the bolt to 10 N·m (89 lb in).

3. Tighten the air cleaner resonator to the throttle body clamp.

Tighten
Tighten the clamp to 5 N·m (44 lb in).

4. Tighten the air cleaner intake duct clamp.

Tighten
Tighten the clamp to 5 N·m(44 lb in).

5. Tighten the vent hose clamp.

Tighten
Tighten the clamp to 2.5 N·m(22 lb in).