For 1990-2009 cars

### Removal Procedure

1. Pull the door weatherstrip away from the garnish molding as required.
2. Pull on the garnish molding to disengage the clips (1) from the windshield pillar.
3. Remove the garnish molding (2) from the car.

### Installation Procedure

1. Position the garnish molding (2) to align the retaining clips.
2. Apply inboard pressure to engage the clips (1) to the windshield pillar.
3. Install the door weatherstrip to the garnish molding as required.