For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Battery Retainer Bolt | 18 N·m | 13 lb ft
Commutator End Frame/Field Frame Assembly Through Bolts | 8.5 N·m | 75 lb in
Front Generator Bracket to Block Attaching Bolt (3.4L) | 50 N·m | 37 lb ft
Generator Rear Mounting Bolt (3.4L) | 25 N·m | 18 lb ft
Ignition Wire Harness Bracket Nut (3.4L) | 13 N·m | 10 lb ft
Ignition Wire Harness Retaining Bolt (3.4L) | 25 N·m | 18 lb ft
Negative Battery to Transaxle Stud Nut | 30 N·m | 22 lb ft
Battery Cable to Battery Bolt (2.4L) | 15 N·m | 11 lb ft
Positive Battery Cable to Generator Nut (3.4L) | 7.5 N·m | 65 lb in
Positive Battery Cable to Starter Solenoid Nut | 12 N·m | 106 lb in
Generator to bracket bolt (2.4L) | 50 N·m | 37 lb ft
Solenoid Attaching Screws | 11 N·m | 95 lb in
Spark Plugs (2.4L) | 19 N·m | 14 lb ft
Spark Plugs (3.4L) | 19 N·m | 14 lb ft
Starter Field Lead to Solenoid Attaching Screw | 9.5 N·m | 84 lb in
Starter Lead Wire to Starter Solenoid S Terminal Nut | 2.5 N·m | 22 lb in
Starter Motor to Engine Bolt (2.4L) | 90 N·m | 66 lb ft
Starter Motor to Engine Bolt (3.4L) | 43 N·m | 32 lb ft