For 1990-2009 cars

Problem | Action
--- | ---
A rattle/buzz noise coming from beneath the back seat area caused by 1 of the following:

• | The rearward most heat shield is not fastened properly. This allows up and down movement of the shield.

• | The park brake cable can be in contact with the heat shield.

• | Fasten the heat shield properly.

• | Adjust the cable in order to remove the contact.

A harsh rattle coming from the front end area. It can also sound like a strut or a thump. | Inspect the front suspension and steering components. Adjust, repair or replace as necessary.
A creaking/popping noise rearward in the vehicle underbody caused by 1 of the following causes:

• | The rear stabilizer bar bushings did not have enough lubricant applied to the bar contact surface.

• | The bushing clamp can be moving in its locating hole.

Apply more lubricant inside of the bushing as well as the clamp.

A hissing noise coming from the trunk compartment/rear strut area caused by the rubber strut cap not being fully seated. This allows strut noise to penetrate the passenger compartment area. | Re-fit the rubber strut cap properly.