For 1990-2009 cars

### Removal Procedure

1. Open the rear compartment lid.
2. With a small flat-bladed tool release the retaining tabs for the seat back release handles.
3. Remove the rear window panel trim. Refer to Rear Window Shelf Trim Panel Replacement in Interior Trim.
4. Remove the seat back release handles from the rear package shelf.
5. Remove the seat back latch bolts from the latch.
6. Remove the seat back latch from the rear package shelf.

### Installation Procedure

1. Install the seat back latch to the rear package self.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the seat back latch bolts to the latch.

Tighten
Tighten the bolts to 25 N·m (18 lb ft).

3. Install the seat back release handles to the rear package shelf.

Press the seat back release handles into the rear package shelf until fully seated.

4. Install the rear window panel trim. Refer to Rear Window Shelf Trim Panel Replacement in Interior Trim.
5. Close the rear compartment lid.
6. Check the seat back latch for proper operations.