For 1990-2009 cars

### Removal Procedure

1. Remove the left instrument panel insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gauges and Console.
2. Disconnect the accelerator cable from the accelerator pedal (1).
3. Disconnect the brake pedal pushrod (1) from the brake pedal (2).
4. Remove the cruise control (2) and brake switch (3) from the brake pedal (1).
5. Disconnect the electrical harness from the brake pedal.
6. Remove the upper (1) and the lower (2) mounting nuts from the brake pedal assembly.
7. Remove the brake pedal assembly (1).

### Installation Procedure

1. Install the brake pedal assembly (1).
2. Install the upper (1) and the lower (2) mounting nuts to the brake pedal assembly.

Tighten
Tighten the mounting nuts to 27 N·m (20 lb in).

3. Connect the electrical harness to the brake pedal.
4. Install the cruise control (2) and brake switch (3) to the brake pedal (1).
5. Connect the brake pedal pushrod (1) to the brake pedal (2).
6. Connect the accelerator cable to the accelerator pedal (1).
7. Install the left instrument panel insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gauges and Console.