For 1990-2009 cars

### Removal Procedure

1. Remove the split/folding rear seat back. Refer to Rear Split Folding Seat Back Replacement .
2. Disconnect hook and loop strip retaining the rear seat cushion cover back and pull back to access the staples.
3. Remove the staples from the cushion cover back.
4. Reach inside of the rear seat back cover in order to unfasten the hook and the loop retainers securing the rear seat back cover to the pad.
5. Remove the rear seat back cover from the seat back, by pulling the seat back cover up and over the pad.

### Installation Procedure

1. Position the rear seat back cover alignment mark to the alignment mark on the pad.
2. Install the hog rings to the rear seat back cover to the pad.
3. Pull the seat back cover over the pad and alining the hook and the loop retainers.
4. Use firm hand pressure in order to fasten the hook and the loop retainers, securing the rear seat back cover to the pad.
5. Install new staples to the cushion cover back.
6. Use firm hand pressure in order to fasten the hook and the loop retainer on the seat back.
7. Install the split/folding rear seat back. Refer to Rear Split Folding Seat Back Replacement .