For 1990-2009 cars

### Front Seat Belt System

Caution: To help avoid personal injury from unrepaired crash damage to a restraint system, perform the seat belt check for each seat belt system. Replace the seat belt system if there is any doubt about the condition of system components.

1. The front seat belt system includes a driver and\or passenger seat belt retractor and buckle.
2. The driver's seat belt system, includes a seat belt switch in the driver seat buckle which controls a reminder lamp and a tone alarm. When the driver seat belt is buckled, the driver's door is closed, and the ignition switch is turned ON, the following events will occur:

• | The tone alarm will not operate.

• | The reminder lamp will not operate.

3. When the driver's seat belt is not buckled, the driver's door is closed, and the ignition switch is in RUN, the following events will occur:

• | The tone alarm will operate for 4 to 8 seconds and then go OFF.

• | The reminder lamp will operate for 20 seconds, until the driver seat belt is buckled.

• | Then the reminder lamp will flash for an additional 55 seconds before going OFF.

• | To diagnose a failure of the reminder lamp or the tone alarm, refer to Diagnostic System Check - Instrument Cluster in Instrument Panel, Gauges and Console.

### Child Seat Restraint System

Caution: A child in a rear-facing child restraint can be seriously injured if the right-front passengers air bag inflates. This is because the back of a rear-facing child restraint would be very close to the inflating air bag. NEVER use a rear-facing child restraint in this vehicle. If a forward-facing child restraint is suitable for your child, ALWAYS move the front passenger seat as far back as it will go and then install the child restraint. Be sure the child restraint position does not conflict with any additional requirements provided by the manufacturer. For more information, refer to the vehicle owners manual and the instruction that came with the child restraint.

The child seat may only be used in a forward facing seating location. The child seat should be installed and secured according to the manufacturer's directions. If the child seat has a top strap it will need to be anchored. Refer to Child Restraint Tether Anchor Replacement .

All vehicles are equipped with a dual-moad type retractor with emergency and automatic locking features. The automatic locking feature is for restraint of a child seat. The child seat can be secured by pulling the seat belt all the way out to lock it. Then, tighten the seat belt around the child seat.

If a child seat is to be used in the second seat position, a special dealer-installed anchor must be used to anchor the child seat top strap. (This only applies to the seats designed with the top strap provision and for the vehicles sold in Canada). In order to assure the correct top strap angle, the child seat is only to be used at the seating position for witch the top strap anchor is installed.