For 1990-2009 cars

### Removal Procedure

1. Remove the rear shelf trim panel. Refer to Rear Window Shelf Trim Panel Replacement in Interior Trim.
2. Remove the foam sound insulators from the rear shelf.
3. Disengage the rear speaker retaining tabs.
4. Remove the rear speaker from the rear shelf.
5. Disconnect the electrical connector from the speakers.

### Installation Procedure

1. Connect the electrical connectors to the rear speaker.
2. Position the rear speaker to the rear shelf.
3. Install the rear speaker. Making sure the plastic speaker tabs engage the rear shelf.
4. Install the foam sound insulators to the rear shelf.
5. Install the rear shelf trim panel. Refer to Rear Window Shelf Trim Panel Replacement in Interior Trim.