For 1990-2009 cars

## Spark Plug Wire Harness Replacement 3.4L

### Removal Procedure

1. Turn the ignition switch to the OFF position.

Notice: Twist the spark plug boot one-half turn in order to release the boot. Pull on the spark plug boot only. Do not pull on the spark plug wire or the wire could be damaged.

2. Note the position of the spark plug wires. Remove the spark plug wires from the front spark plugs by twisting the boot ½ turn before removing the spark plug boots.
3. Note the position of the spark plug wire retaining clips (2). Remove the spark plug wire retaining clips from the engine.
4. Rotate the engine forward.
5. Remove the spark plug wire(s) from the rear spark plug(s).
6. Remove the spark plug wire retaining clips (3) from the rear of the engine.
7. Remove the spark plug wires from the ignition coils.
8. Remove the spark plug wires from the engine.
9. If replacing the spark plug wires, transfer any of the following:

• | Boot heat shields

• | Spark plug wire conduit

• | Spark plug wire retaining clips (2)

### Installation Procedure

1. Install the spark plug wires to the engine.
2. Install the spark plug wires to the ignition coils.
3. Install the spark plug wires to the rear spark plugs.
4. Install the spark plug wire retaining clips (3) at the rear of the engine.
5. Return the engine to the proper position.
6. Install the spark plug wires to the front spark plugs.
7. Install the spark plug wire retaining clips (2) to the front of the engine.