For 1990-2009 cars

### Removal Procedure

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise the vehicle. Support the vehicle.
2. Loosen the oil pan bolts.
3. Drain the oil. Use a suitable container to catch the transmission fluid.
4. Remove the oil pan attaching bolts.
5. Remove the oil pan.
6. Remove the oil pan gasket.

### Installation Procedure

1. Clean and inspect the oil pan for dents or damage. Dry the oil pan before installation.
2. Install the oil pan gasket. Use a new gasket if the sealing ribs are damaged.
3. Install the oil pan. Replace the bottom pan if damaged.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the oil pan attaching bolts.

Tighten
Tighten the bolts to 12 N·m (106 lb in).

5. Lower the vehicle.
6. Check the pan for leaks. Refill the transmission to the proper level with DEXRON®-III. Refer to Fluid Capacity Specifications .
7. Recheck the fluid level. Refer to Transmission Fluid Check .
8. Inspect the oil pan gasket for leaks.