For 1990-2009 cars

### Removal Procedure

1. Remove the rear seatback. Refer to Rear Seat Back Replacement .
2. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement .
3. Remove the lock pillar lower trim panel retainer (2).
4. Remove the lock pillar lower trim panel (1) by disengaging the tabs from the clips.

### Installation Procedure

1. Install the lock pillar lower trim panel (1):

1.1. | Align and engage the lock pillar lower trim panel tabs to the clips.

1.2. | Apply pressure to the lock pillar lower trim panel in order to fully engage the tabs.

2. Install the lock pillar lower trim panel retainer (2).
3. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement .
4. Install the rear seatback. Refer to Rear Seat Back Replacement .