For 1990-2009 cars

### Removal Procedure

Important: Securely latch the seat back in the full forward position before removal.

1. Remove the J-retainer from the seat back cover.
2. Lift up on the recliner handle in order to dump the seat back to the full forward position. This action will release the recliner.
3. Pull back on the seat back without lifting the handle. The recliner will latch the seat back into the full forward position.
4. Raise the seat back cover trim in order to gain access to the seat recliner to seat back bolts (2).
5. Remove the seat recliner bolt from the seat back pad assembly (1).
6. Remove the seat back (1) from the recliner mechanisms (3).

### Installation Procedure

Important: Correctly align the seat back frame with the recliner. Once the seat back holes are aligned with the recliner holes, do not lean on the seat back. This action may cause the seat back to twist or to misalign. Twists or misalignments may cause the recliner system to fail.

1. Install the seat back (1) to the recliner mechanisms (3).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the seat recliner bolts to (2) the seat back.

Tighten
Tighten the bolts to 3 N·m (27 lb in).

3. Install the J-retainer seat back cover.