For 1990-2009 cars

#### Tools Required

J 37059 Accessory Drive Belt Tensioner Wrench

### Removal Procedure

Caution: To avoid personal injury when rotating the accessory drive belt tensioner, use a tight fitting 13 mm wrench that is at least 46 cm (18 in) long.

1. Rotate the drive belt tensioner using the J 37059 .
2. Remove the drive belt.

### Installation Procedure

1. Rotate the drive belt tensioner using the J 37059 .
2. Install the drive belt.