For 1990-2009 cars

### Removal Procedure

1. Remove the seat back bolster. Refer to Rear Split Folding Seat Back Bolster Replacement .
2. Pull the bolster cover over the U-bracket.
3. Remove the bolster cover from the pad by pulling the cover up and over the pad.

### Installation Procedure

1. Position the back bolster cover onto the pad.
2. Install the back bolster cover by pulling down and over the pad.
3. Pull the bolster cover over the U-bracket.
4. Install the seat back bolster. Refer to Rear Split Folding Seat Back Bolster Replacement .