For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Exhaust Crossover Pipe Bolt | 25 N·m | 18 lb ft
Exhaust Crossover Pipe Heat Shield Bolt | 10 N·m | 89 lb in
Exhaust Manifold Brace to Exhaust Manifold Bolt | 56 N·m | 41 lb ft
Exhaust Manifold Brace to Exhaust Manifold Nut | 26 N·m | 19 lb ft
Exhaust Manifold Heat Shield Bolt (2.4L) | 14 N·m | 10 lb ft
Exhaust Manifold Heat Shield Bolt (3.4L) | 10 N·m | 89 lb in
Exhaust Manifold Nut (2.4L) | 13 N·m | 110 lb in
Exhaust Manifold Nut (3.4L) | 16 N·m | 12 lb ft
Exhaust Muffler Inlet Pipe Clamp Nut | 50 N·m | 37 lb ft
Flex Decoupler to Exhaust Manifold Bolt | 35 N·m | 26 lb ft