For 1990-2009 cars

### Removal Procedure

1. Raise the head restraint to the highest position.
2. Remove the seat belt strap from the guide, if required.
3. Insert a small flat-bladed tool onto the tab on the side of the guides.

Pressing in one tab at a time while slightly pulling up on that side.

4. Remove the head restraint by pulling upward and out.

### Installation Procedure

1. Position the head restraint to the guides in the seat back.
2. Instal the head restraint pressing down until the head restraint stops at the detent.
3. Reposition the head restraint to the original position.
4. Install the seat belt strap to the guide, if required.