For 1990-2009 cars

### Removal Procedure

1. Remove the front seat. Refer to Front Seat Replacement - Bucket .
2. Squeeze the oblong connector (1, 2) for the vertical and the horizontal drive cables.
3. Pull outward on the cable to remove from the following locations:

• | The motors

• | The vertical and horizontal actuators

### Installation Procedure

1. Install the cables to the following locations:

• | The motors

• | The vertical and horizontal actuators

2. Push the connectors (1, 2) into the actuators and the motors until a loud audible click is heard.
3. Install the front seat. Refer to Front Seat Replacement - Bucket .