For 1990-2009 cars

The vehicle theft deterrent (VTD) system functions are provided by the theft deterrent control module. The VTD system prevents vehicle operation if a valid, learned transponder passkeyIII (PK3) ignition key is not used to start the vehicle. The PK3 key has a transponder embedded in the plastic head of the key. The exciter is an antenna which is made up of wire coils which surround the ignition lock cylinder. The PCM enables engine starting when it receives a valid (learned) password from the theft deterrent control module via the class 2 serial data circuit. The components of the VTD system are as follows:

• | Theft deterrent control module

• | Powertrain control module (PCM)

• | Ignition key (Transponder)

• | Ignition lock cylinder

• | Security indicator

### Theft Deterrent Control Module

Vehicles with steering column mounted ignition switches have the exciter integral with the theft deterrent control module which is located within the steering column. Vehicles with instrument panel mounted ignition switches have exciter modules separate from the theft deterrent control module with the vehicle wiring harness connecting the two. The theft deterrent control module for vehicles with instrument panel mounted ignition switches is located within the instrument panel. The theft deterrent control module can learn up to ten keys (transponder values).

The theft deterrent control module uses the following inputs, battery voltage, ignition switched voltage and ground circuit. The theft deterrent control module uses the following outputs, password exchange with the PCM (fuel enable/disable) via class 2 serial data circuit.

When an ignition key is inserted into the ignition lock cylinder, the transponder embedded in the head of the key is energized by the exciter coils surrounding the ignition lock cylinder. The energized transponder transmits a signal that contains its value, which is received by the theft deterrent control module. The theft deterrent control module then compares this value to a value stored in memory and performs one of the following functions:

• | If the transponder value is correct, the theft deterrent control module sends a class 2 message containing the module's enable password to the PCM.

• | If the transponder value is incorrect, the theft deterrent control module sends a class 2 message containing a disable password to the PCM.

• | If the theft deterrent control module is unable to measure the ignition key transponder value for 1 second, due to a damaged or missing pellet or a damaged exciter, it sends a class 2 message containing a disable password to the PCM.

### Powertrain Control Module (PCM)

The PCM verifies that the password received from the theft deterrent control module via the Class 2 serial data circuit is correct. The theft deterrent control module can learn only one enable password. If the enable password is correct, the PCM enables the starting and fuel delivery systems.

The PCM disables the starting and fuel delivery systems if any of the following conditions occur:

• | The enable password is incorrect.

• | The system disable password is sent by the theft deterrent control module.

• | No passwords are received - there is no communication with the theft deterrent control module.

### The Ignition Key (Transponder)

The ignition key for theft deterrent equipped vehicles is a typical looking ignition key with a transponder located in the plastic end of the key. The transponder value is fixed and unable to be changed. The theft deterrent system uses the ignition key transponder value to determine if a valid ignition key is being used to start the vehicle. There are approximately three trillion possible transponder values. There are no visible electrical contacts. The keys may be identified by the letters "PK3" stamped into the steel shank of the key. The theft deterrent systems use the following types of ignition keys:

#### Master Keys

Master keys (black plastic end) are for full access operation of the vehicle. Master keys may perform the following functions:

• | Start the vehicle.

• | Lock/unlock all of the door locks.

• | Lock/unlock all of the storage compartments.

### Ignition Lock Cylinder

The ignition lock cylinder performs all of the functions of a lock cylinder on a non PK3 equipped vehicle. The ignition lock cylinder for vehicles with PK3 may be located on the steering column or on the instrument panel. In either location the exciter coils surround the ignition lock cylinder such that they are very close to the head of the key which contains the transponder pellet.

If an ignition lock cylinder is replaced, the PK3 keys must match the mechanical coding of the new lock cylinder. When replacing an ignition lock cylinder, and new PK3 keys are required, refer to Programming Theft Deterrent System Components .

### SECURITY Indicator Operation

The theft deterrent control module can command the instrument cluster to illuminate the SECURITY indicator only when the ignition key is in the ON position. If the PCM loses communication with the theft deterrent control module, the instrument cluster will also detect the loss of communication and will illuminate the SECURITY indicator. The SECURITY indicator can indicate both malfunctions (Indicator on steady) and tamper (Indicator flashing - indicating unauthorized operation). Under the following conditions the SECURITY indicator may be commanded to illuminate.

#### SECURITY Indicator Stays Illuminated and Engine Starts

If the theft deterrent control module was unable to measure the ignition key transponder value or the PCM lost communication with the theft deterrent control module while the engine was last running, the indicator will remain illuminated during subsequent ignition cycles. This is to remind the driver that the vehicle theft deterrent system will not be functioning until the problem is corrected.

#### SECURITY Indicator Illuminates when Engine is Running

If the theft deterrent control module is unable to measure the ignition key transponder value or the PCM loses communication with the theft deterrent control module while the engine is running, the indicator will be illuminated.

#### SECURITY Indicator Illuminated and Engine Does Not Start

The theft deterrent control module or the PCM has detected a problem with the theft deterrent system. The theft deterrent control module is unable to measure the ignition key transponder value. The System is in Learn Mode, refer to Programming Theft Deterrent System Components .

#### SECURITY Indicator Flashes and Engine Does Not Start

The theft deterrent control module has measured an incorrect transponder value when the ignition key is turned to the ON position. The transponder has not been learned by the theft deterrent control module. This is considered a tamper condition by the theft deterrent control module.