For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the engine front cover. Refer to Engine Front Cover Replacement .

Notice: The engine front cover could be damaged if it is not properly supported during seal removal.

3. Support the front cover and drive the oil seal out the timing chain side of the cover.

### Installation Procedure

#### Tool Required

J 36010 Front Cover Crankshaft Seal Installer

1. Using J 36010 , position the seal into the front cover by driving the seal from the timing chain side.
2. Install the engine front cover. Refer to Engine Front Cover Replacement .
3. Connect the negative battery cable.