For 1990-2009 cars
Engine Controls Components
Engine Data Sensors
OBD II Symbol Description Notice
Handling ESD Sensitive Parts Notice

### Circuit Description

The intake air temperature (IAT) sensor is a thermistor which measures the temperature of the air entering the engine. The powertrain control module (PCM) applies 5.0 volts through a pull up resistor to the IAT sensor. When the intake air is cold, the sensor resistance is high and the PCM will monitor a high signal voltage on the IAT signal circuit. If the intake air is warm, the sensor resistance is lower causing the PCM to monitor a lower voltage. DTC P1112 will set when the PCM detects an intermittently low signal voltage on the intake air temperature sensor signal circuit.

### Conditions for Running the DTC

• | No active ECT, MAF Sensor, or VSS DTCs.

• | The engine has been running for over 10 seconds.

• | Vehicle speed is more than 25 mph.

### Conditions for Setting the DTC

• | The IAT sensor indicates an intake air temperature intermittently more than 135°C (275°F).

• | The condition is present for up to 5 seconds.

### Action Taken When the DTC Sets

The PCM stores conditions which were present when the DTC set as Failure Records only. This information will not be stored as Freeze Frame Records.

### Conditions for Clearing the MIL/DTC

• | The DTC becomes history when the conditions for setting the DTC are no longer present.

• | The history DTC clears after 40 malfunction free warm-up cycles.

• | The PCM receives a clear code command from the scan tool.

### Diagnostic Aids

Inspect for the following conditions:

Many situations may lead to an intermittent condition. Perform each inspection or test as directed.

Important: : Remove any debris from the connector surfaces before servicing a component. Inspect the connector gaskets when diagnosing or replacing a component. Ensure that the gaskets are installed correctly. The gaskets prevent contaminate intrusion.

• | Loose terminal connection

- | Use a corresponding mating terminal to test for proper tension. Refer to Testing for Intermittent Conditions and Poor Connections , and to Connector Repairs in Wiring Systems for diagnosis and repair.

- | Inspect the harness connectors for backed out terminals, improper mating, broken locks, improperly formed or damaged terminals, and faulty terminal to wire connection. Refer to Testing for Intermittent Conditions and Poor Connections , and to Connector Repairs in Wiring Systems for diagnosis and repair.

• | Damaged harness--Inspect the wiring harness for damage. If the harness inspection does not reveal a problem, observe the display on the scan tool while moving connectors and wiring harnesses related to the sensor. A change in the scan tool display may indicate the location of the fault. Refer to Wiring Repairs in Wiring Systems for diagnosis and repair.

• | Inspect the powertrain control module (PCM) and the engine grounds for clean and secure connections. Refer to Wiring Repairs in Wiring Systems for diagnosis and repair.

If the condition is determined to be intermittent, reviewing the Snapshot or Freeze Frame/Failure Records may be useful in determining when the DTC or condition was identified.

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Powertrain On Board Diagnostic (OBD) System Check? | -- | Go to Step 2 | Go to Powertrain On Board Diagnostic (OBD) System Check
2 | With a scan tool, select Diagnostic Trouble Codes (DTC). Does the scan tool indicate DTC P0112 also set? | -- | Go to DTC P0112 Intake Air Temperature (IAT) Sensor Circuit Low Voltage | Go to Step 3
3 | Test the signal circuit for an intermittent short to ground. Refer to Testing for Intermittent Conditions and Poor Connections and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | -- | Go to Step 4 | Go to Diagnostic Aids
4 |

1. Use the scan tool in order to clear the DTCs.
2. Operate the vehicle within the Fail Record conditions as noted.

Does the DTC reset?

--

Go to Step 2

System OK