For 1990-2009 cars

### Removal Procedure

1. Remove the front carpet. Refer to Front Floor Panel Carpet Replacement in Interior Trim.
2. Remove the right side rear floor air outlet from the stud.
3. Remove the right side rear floor air outlet from the left side rear floor air outlet.
4. Remove the left side rear floor air outlet from the stud.
5. Remove the left side rear floor air outlet from the floor air outlet.

### Installation Procedure

1. Install the left side rear floor air outlet to the floor air outlet.
2. Install the left side rear floor air outlet on the stud.
3. Install the right side rear floor air outlet to the left side rear floor air outlet.
4. Install the right side rear floor air outlet on the stud.
5. Install the front carpet. Refer to Front Floor Panel Carpet Replacement in Interior Trim.