For 1990-2009 cars

Important:

• | Store the valve lifters so that they can be installed in the same bore from which they were removed.

• | Do not disassemble the valve lifter.

• | Do not apply force to the body (valve side) of the valve lifter, this will force oil to leak out of the valve lifter.

• | Store the valve lifters submerged in clean engine oil camshaft side down until installation.

• | Store the valve lifters camshaft side up if left in air until installation. Do not store in air with the camshaft side down or on the valve lifter side.

1. Remove the lifters.