For 1990-2009 cars

#### Tools Required

J 36850 TRANSJEL™

1. Assemble the input carrier assembly (562) to the reaction internal gear (560.
2. Retain the input carrier assembly with the snap ring (563).
3. Assemble the thrust bearing (107) onto the input carrier assembly.
4. Retain the thrust bearing with J 36850 or equivalent. You will find another thrust bearing permanently retained in the input carrier assembly (562).