For 1990-2009 cars

### Removal Procedure

The rearview mirror fastens to the mirror support that bonds to the windshield.

1. Disconnect the rearview mirror reading lamp electrical connector, if applicable.
2. Loosen the set screw.
3. Slide the rearview mirror upward from the support.

### Installation Procedure

1. Ensure that the set screw will clear the rearview mirror support.
2. Slide the rearview mirror assembly downward on the support until the mirror assembly bottoms.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the rearview mirror set screw.

Tighten
Tighten the rearview mirror set screw to 2 N·m (18 lb in).

4. Install the rearview mirror reading lamp electrical connector, if applicable.