For 1990-2009 cars

### Removal Procedure

1. Remove the right headlamp assembly. Refer to Headlamp Assembly or Headlamp Bulb and/or Cornering, Sidemarker, Park, Turn Signal Bulb Replacement in Lighting Systems.
2. Disconnect the horn electrical connector.
3. Remove the horn bracket bolt.
4. Remove the horn from the front frame rail.

### Installation Procedure

1. Position the horn to the front frame rail.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the horn bracket bolt.

Tighten
Tighten the bolt to 10 N·m (89 lb in).

3. Connect the horn electrical connector.
4. Install the right headlamp assembly. Refer to Headlamp Assembly or Headlamp Bulb and/or Cornering, Sidemarker, Park, Turn Signal Bulb Replacement in Lighting Systems.