For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the transaxle assembly from the vehicle. Refer to Transmission Replacement .
3. Remove the torque convertor assembly from the transaxle.
4. Remove the torque convertor O-ring seal from the end of the turbine shaft. Use a screwdriver.

### Installation Procedure

1. Install a new torque convertor O-ring seal on the end of the turbine shaft.
2. Install the torque convertor onto the transaxle.
3. Install the transaxle into the vehicle. Refer to Transmission Replacement .
4. Connect the negative battery cable.
5. Adjust the oil level.