For 1990-2009 cars

1. Drain the engine oil.
2. Remove the throttle body and intake manifold. Refer to Intake Manifold Replacement .
3. Remove the left and right cylinder head covers. Refer to Camshaft Cover Replacement - Left Side and Camshaft Cover Replacement - Right Side .
4. Remove the water pump pulley.
5. Remove the water pump drive belt.
6. Remove the 3 bolts and the thermostat cap.
7. Remove the 3 bolts from the power steering pump bracket and remove bracket.
8. Remove the crankshaft balancer. Refer to Crankshaft Balancer Replacement .
9. Remove the lower oil pan. Refer to Lower Oil Pan Removal .
10. Remove the upper oil pan. Refer to Upper Oil Pan Removal
11. Disconnect the crankshaft position (CKP) sensor connector.
12. Remove the bolt and the crankshaft position (CKP) sensor.
13. Remove the bolts and the front cover (1).