For 1990-2009 cars

### Removal Procedure

1. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement in Engine Controls-2.2L. Refer to Air Cleaner Assembly Replacement in Engine Controls-3.4L.
2. Remove and set aside the under hood electrical center. Refer to Underhood Electrical Center or Junction Block Replacement in Wiring Systems.
3. Remove the battery tray. Refer to Battery Tray Replacement .
4. Release the wiring harness retainers and set the wiring harness aside.
5. Move the engine heater cable aside, if equipped.
6. Remove the bracket to strut tower bolts from the air cleaner and electrical center mounting bracket.
7. Remove the bracket to body bolts from the air cleaner and electrical center mounting bracket.
8. Remove the mounting bracket from the vehicle.

### Installation Procedure

1. Position the mounting bracket to the vehicle.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bracket to body bolts to the air cleaner and electrical center mounting bracket.

Tighten
Tighten the air cleaner bracket bolts to 10 N·m (89 lb in).

3. Install the bracket to strut tower bolts to the air cleaner and electrical center mounting bracket.

Tighten
Tighten the bracket to strut tower bolts to 10 N·m (89 lb in).

4. Place the wiring harness into position and secure the wiring harness retainers.
5. Install the under hood electrical center. Refer to Underhood Electrical Center or Junction Block Replacement in Wiring Systems.
6. Install the battery tray. Refer to Battery Tray Replacement .
7. Install the air cleaner assembly. Refer to Air Cleaner Assembly Replacement , in Engine Controls 2.2L. Refer to Air Cleaner Assembly Replacement , in Engine Controls 3.4L.