For 1990-2009 cars

### Removal Procedure

1. Remove the right front wheelhouse panel splash shield. Refer to Wheelhouse Splash Shield Replacement .
2. Remove the left front wheelhouse panel splash shield. Refer to Wheelhouse Splash Shield Replacement .
3. Remove the fender to fascia retaining push pins.
4. Remove the fender to fascia retaining bolts.
5. Remove the retainers (2) from the top of the fascia (4).
6. Remove the retainers (5) from the bottom of the fascia (4).
7. Remove the fascia (4) from the impact bar (6).

### Installation Procedure

1. Install the fascia (4) to the impact bar (6).
2. Install the retainers (2) to the top of the fascia (4).
3. Install the retainers (5) to the bottom of the fascia (4).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the fender to the fascia retaining bolts.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

5. Install the fascia to the fender retaining push pins.
6. Install the left front wheelhouse panel splash shield. Refer to Wheelhouse Splash Shield Replacement .
7. Install the right front wheelhouse panel splash shield. Refer to Wheelhouse Splash Shield Replacement .