For 1990-2009 cars

Caution: To avoid any vehicle damage, serious personal injury or death when major components are removed from the vehicle and the vehicle is supported by a hoist, support the vehicle with jack stands at the opposite end from which the components are being removed and strap the vehicle to the hoist.

1. Raise the vehicle.
2. Disconnect the fuel pump electrical connector.
3. Lower the vehicle.
4. Start and run the engine until the fuel supply remaining in the fuel pipes is consumed. Engage the starter for 3.0 seconds in order to assure relief of any remaining pressure.
5. Raise the vehicle.
6. Connect the fuel pump electrical connector.
7. Lower the vehicle.
8. Disconnect the negative battery cable in order to avoid possible fuel discharge if an accidental attempt is made to start the engine.