For 1990-2009 cars

### Removal Procedure

Important: Mark the location and the color of the wires to the electrical socket before removing the wires.

1. Remove the conduit from the center pillar.
2. Disconnect the rear door wiring harness electrical connector from the body harness.
3. Disconnect the wire harness retainer from the wiring harness socket.
4. Remove the wiring harness wiring one at a time from the socket.
5. Remove the rubber conduit from the rear door.
6. Remove the wiring harness wiring from the rubber conduit.

### Installation Procedure

1. Install the rear door electrical harness through the rubber conduit.
2. Install the rear door wiring harness wires to the electrical socket.
3. Connect the rear door wiring harness electrical connector.
4. Install the rubber conduit to the rear door.
5. Install the rubber conduit to the center pillar.