For 1990-2009 cars

### Diagnostic Aids

The clutch is noisy when the clutch is fully engaged. In some cases there might be improper pedal travel, faulty pilot bearing, driven disc or even the clutch hub binding on the gear spline.

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. This step explains there parts and the operation of the clutch system.

2. This step checks for worn or damaged parts.

Step | Action | Yes | No
--- | --- | --- | ---
DEFINITION: The clutch is noisy with the clutch fully engaged.
1 | Did you review the clutch symptom operations and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Clutch
2 |

1. Inspect for a worn or damaged release bearing.
2. Remove the transmission. Refer to Transmission Replacement .

Is the release bearing worn or damaged?

Go to Step 3

System OK

3 | Replace the release bearing assembly. Refer to Clutch Pressure and Driven Plate Replacement . Is the release bearing still noisy? | Go to Step 4 | System OK
4 | Check for a worn or loose pilot bearing. Is the pilot bearing worn or loose? | Go to Step 5 | System OK
5 | Replace the pilot bearing. Refer to Engine Flywheel Replacement in Engine Mechanical 2.2L (L61) or Engine Flywheel Replacement in Engine Mechanical 3.4L. Did you find and repair the condition? | Go to Step 6 | Go to Diagnostic Aids
6 |

1. Install the transmission. Refer to Transmission Replacement .
2. Operate the system in order to verify the repair.

Did you correct the condition?

System OK

Go to Step 1